################################################################################################
## Configuration template for GXV-3000 firmware version 1.1.3.14
################################################################################################

##############################################################################
##  Advanced/System-wide Options
##############################################################################

# Password for configuration file authentication
P1 = 

# Admin password for web interface, max. length is 30
P2 = sarabon

# G.723 rate: 0 - 6.3kbps encoding rate,  1 - 5.3kbps encoding rate
P49 = 

P86 = 6

# Silence Suppression. 0 - no, 1 - yes
P50 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively)
P37 = 2

# Video frame rate: default - 15
P904 = 15

# Video bit rate (kbps): default is 128
P905 = 128

# Video Packet Size: maxlength = 4, from 100~1400, default is 1400
P927 = 800

# Video Rate Control. 0 - Frame, 1 - TMN8
P924 =

# Video Frame Skipping. 0 - no, 1 - yes
P925 = 0

# Sharpening Filter. (0-9, 0 means disabled, default is 5) 
P938 = 5

# Brightening Filter.  (0-9, 0 means disabled, default is 5)
P939 = 5

# Tone Remapping Filter. (0-255, 0 means disabled, default is 32)
P948 = 32

# Enable Video Surveillance. Turn phone into video surveillance camera if set to 1, YES. Default=No, 0.
P928 = 0

# Surveillance RTSP Port.  Video Surveillance data stream port, default is 554.
P929 = 554

# Streaming RTSP Server
P953 =

# Streaming RTSP User ID
P954 =

# Streaming RTSP Password
P955 =

# Layer 3 QoS (IP Diff-Serv or Precedence value for RTP)
P38 = 0

# Layer 2 QoS. 802.1Q/VLAN Tag (VLAN classification for RTP)
P51 = 0

# Layer 2 QoS. 802.1p priority value (0 - 7)
P87 = 0

# No Key Entry Timeout. Default - 4 seconds.
P85 = 4

# Use # as Dial Key. 0 - no, 1 - yes
P72 = 1

# Local RTP port (1024-65535, default 5004)
P39 = 5004 

# Use Random Port. 0 - no, 1 - yes
P78 = 0

# Keep-alive interval (in seconds. default 20 seconds)
P84 = 60

# Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. Example 64.3.153.50.
P101 =

# STUN server
P76 = stun.mycompany.com

#-------------------------------------------------------------
# Firmware Upgrade
#-------------------------------------------------------------

# Firmware Upgrade. 0 - TFTP Upgrade,  1 - HTTP Upgrade.
P212 = 0

# Firmware Server Path
# P192 = fm.grandstream.com/gs
P192 = 192.168.45.5

# Config Server Path
# P237 = fm.grandstream.com/gs
P237 = 192.168.45.5

# Firmware File Prefix
P232 =

# Firmware File Postfix
P233 =

# Config File Prefix
P234 =

# Config File Postfix
P235 =

# Allow DHCP Option 66 to override server. 0 - No, 1 - Yes. Default is Yes.
# When set to Yes(1), it will override the configured provision path and method.
P145 = 1

# Automatic Upgrade. 0 - No, 1 - Yes. Default is No.
P194 = 0

# Check for new firmware every () minutes, unit is in minute, minimnu 60 minutes, default is 7 days.
P193 = 10080

# Use firmware pre/postfix to determine if f/w is required
# 0 = Always Check for New Firmware 
# 1 = Check New Firmware only when F/W pre/suffix changes
# 2 = Always Skip the Firmware Check
P238 = 0

# Authenticate Conf File
P240 = 0

# Enable Screen Saver Download
# 0 = No
# 1 = YES, HTTP
# 2 = YES, TFTP 
P933 = 0

# Screen Saver Download Server Path
P934 =

# Enable Phonebook XML Download
# 0 = No
# 1 = YES, HTTP
# 2 = YES, TFTP
P330 = 0

# Phonebook XML Server Path
# This is a string of up to 128 characters that should contain a path to the XML file.  
# It MUST be in the host/path format. For example: "directory.grandstream.com/engineering"
P331 =

# Remove Manually-edited entries on Download
# 0 - No, 1 - Yes
P333 = 0

# Enable Network Screen Saver
# 0 - No
# 1 - YES, HTTP 
P943 = 0

# Network Screen Saver Server Path
P942 =

# Enable Weather Forecast
# 0 - No
# 1 - YES, HTTP
P945 = 0

# Weather Forecast Server Path
P944 =

# Enable Headline News
# 0 - No
# 1 - YES, HTTP
P947 = 0

# Headline News RSS Server Path
P946 =

# Offhook Auto Dial
P71 = 

# DTMF Payload Type
P79 = 101

# Syslog Server (name of the server, max length is 64 charactors)
P207 = 

# Syslog Level (Default setting is NONE)
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR
P208 = 0

# NTP Server
P30 = ntp.bring.out.ba

# Allow DHCP Option 42 to override NTP server. 0 - No, 1 - Yes. Default is No.
# When set to Yes(1), it will override the configured NTP server.
P144 = 0

# Distinctive Ring Tone
# Use custom ring tone 1 if incoming caller ID is the following:
P105 =

# Use custom ring tone 2 if incoming caller ID is the following:
P106 =

# Use custom ring tone 3 if incoming caller ID is the following:
P107 =

# System Ring Tone:  input type = text, maxlength=64 size=30  
P345 = f1=440,f2=480,c=200/400;

#------------------------------------------------------------
#Call Progress Tones: input type=text, maxlength=64, size=30
#------------------------------------------------------------

# Dial Tone        
P343 = f1=350,f2=440;

# Message Waiting Tone
P344 = f1=350,f2=440,c=10/10;

# Ring Back Tone
P346 = f1=440,f2=480,c=200/400;

# Call-Waiting Tone
P347 = f1=440,f2=440,c=25/525;

# Busy Tone
P348 = f1=480,f2=620,c=50/50;

# Reorder Tone
P349 = f1=480,f2=620,c=25/25;

# Start Browser On Boot:    0 - no (default), 1 - yes
P950 = 0

# Enable Browser Toolbar:   0 - no (default), 1 - yes
P951 = 0

# Browser Home Page, maxlength=64, default = about:/start.htm
P952 = about:/start.htm

# Disable Call Waiting. 0 - no, 1 - yes
P91 = 0

# Disable Call Waiting Tone: 0 - no (default), 1 - yes
P186 = 0

# Disable Direct IP Call. 0 - no, 1 - yes
P277 = 0

# Use Quick IP-call mode: 0 - no, 1 - yes. Default is No.
P184 = 0

# Allow Media Loopback. 0 - no, 1 - yes
P278 = 0

# Lock Keypad Update. 0 - no, 1 - yes
P88 = 0

# Display Language. 0 - English, 1 - Downloaded Language, 2 - Chinese
P342 = 0

# language file postfix
P399 =

####################################################################
# Primary Account (Account 1) Settings
####################################################################

# Account Active (In Use). 0 - no, 1 - yes
P271 = 1

# Account Name
P270 = 20

# SIP Server: max. length = 96
P47 = asterisk.bring.out.ba

# Outbound Proxy
P48 = asterisk.bring.out.ba

# SIP User ID
P35 = 20

# Authenticate ID
P36 = 20

# Authenticate password
P34 = sarabon

# Display Name (John Doe)
P3 = hernad dish 

# Use DNS SRV. 0 - No, 1 - Yes.
P103 = 0

# SIP User ID is phone number. 0 - no, 1 - yes
P63 = 0

# SIP Registration. 0 - no, 1 - yes
P31 = 1

# Unregister On Reboot. 0 - no, 1 - yes
P81 = 1

# Register Expiration (in minutes. default 1 hour, max 45 days)
P32 = 10

# SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 20)
P138 = 20

# Local SIP port (default 5060)
P40 = 5060

# NAT Traversal (STUN). 0 - yes, 1 - no, 2 - No, but send keep-alive
P52 = 1

# SUBSCRIBE for MWI. (Whether or not send SUBSCRIBE for Message Waiting Indication) 0 - No, 1 - Yes.
P99 = 0

# Proxy-Require (A SIP extension to enable firewall penetration)
P197 =

# SIP Compact Header. 0 - no, 1 - yes
P289 = 0

# Voice Mail UserID (User ID/extension for 3rd party voice mail system)
P33 =

# Send DTMF. 8 - in audio, 1 - via RTP, 2 - via SIP INFO, 11 - In Audio & RTP & SIP INFO
# 9 - In Audio & RTP, 10 - IN Audio & SIP INFO, 3 - RTP & SIP INFO
P73 = 8

# Early Dial (use "Yes" only if proxy supports 484 response). 0 - no, 1 - yes
P29 = 0

# Dial Plan Prefix (dial plan prefix string)
P66 =

# Dial Plan. Maxlength = 128 character. Defalut is allow all, {x.}, see user manual
P290 ={x+}                                                                                                           

# Delayed Call Forward Wait Time. Default is 20 seconds, maxlength = 5 
P139 = 20

# Enable Call Features.  0 - no, 1 - yes
P191 = 1

# Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
P260 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
P261 = 90

# Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
P263 = 0

# Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
P264 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
P267 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
P265 = 0

# Enable 100rel. 0 - no, 1 - yes
P272 = 0

# Account Ring Tone. 0 - system ring tone, 1 - custom ring tone 1, 2 - custom ring tone 2, 3 - custom ring tone 3.
P104 = 0

# Send Anonymous. 0 - no, 1 - yes (caller ID will be blocked if set to Yes)  
P65 = 0

# Anonymous Call Rejection:  0 - no (default),  1 - yes 
P129 = 0

# Refer-To Uses Target Contact:  0 - no (default),  1 - yes 
P135 = 0

# Auto Answer. 0 - no, 1 - yes, 2 - Intercom/Paging
P90 = 0

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 3 - GSM, 4 - G.723.1, 8 - PCMA, 
# 9 - G.722, 18 - G.729A/B, 98 - iLBC

# Currently only PCMU/PCMA, GSM, G.723, G.729 and G.726-32 supported, will add others in the future 

# First codec.   
P57 = 0

# Second codec.  
P58 = 8

# Third codec. 
P59 = 4

# Forth codec.  
P60 = 18

# Fifth codec.
P61 = 3

# Sixth codec.
P62 = 2

# Seventh codec.
P46 = 0

# Eighth codec.
P98 = 0

# Preferred Video Coder:   99 - H.264, 34 - H.263, 103 - H.263+ (1998)
# Choice 1
P295 = 99

# Choice 2
P296 = 34

# Jitter Delay: 0 - Medium, 1 - Low, 2 - High
P300 = 0 

# Enable Video: 0 - No, 1 - Yes
P292 = 1

# H.264 payload type: between 96 ~ 127, default = 99
P293 = 99

# H.263+ (1998) payload type: between 96 ~ 127, default = 103
P350 = 103

# SRTP Mode: Disabled - 0, Enabled but not forced - 1, Enabled and forced - 2
P183 = 0

# Special Feature.    100 - Standard, 101 - Nortel MCS, 102 - BroadSoft, 104 - Sonus, 108 - CBCOM, 109 - RNK
P198 = 100

########################################################################
# SIP Account 2 Settings
########################################################################

# Account Active (In Use). 0 - no, 1 - yes
P401 = 0

#Account Name
P417 = 

# SIP Server
P402 =

# Outbound Proxy Server
P403 =

# Account 2 SIP User ID
P404 =

# Authenticate ID
P405 =

# Authenticate Password
P406 =

# Display Name (John Doe)
P407 =

# Use DNS SRV. 0 - No, 1 - Yes.
P408 = 0

# User ID is phone number; "user=phone". 0 - no, 1 - yes
P409 = 0

# SIP Registration. 0 - no, 1 - yes
P410 = 1

# Unregister on Reboot. 0 - no, 1 - yes
P411 = 0

# Register Expiration (in minutes. default 1 hour, max 45 days)
P412 = 60

# Registration Retry Wait Time (in seconds. Between 1-3600, default is 20)
P471 = 20

# Local SIP port (default 5062)
P413 = 5062

# NAT Traversal. 0 - yes, 1 - no, 2 - No, but send keep-alive
P414 = 0

# Subscribe MWI. (Whether or not send SUBSCRIBE for Message Waiting Indication) 0 - No, 1 - Yes.
P415 = 0

# Proxy Require
P418 =

# SIP Compact Header. 0 - no, 1 - yes
P472 = 0

# Voice Mail UserID (User ID/extension for 3rd party voice mail system)
P426 =
 
# Send DTMF. 8 - in audio, 1 - via RTP, 2 - via SIP INFO, 11 - In Audio & RTP & SIP INFO
# 9 - In Audio & RTP, 10 - IN Audio & SIP INFO, 3 - RTP & SIP INFO
P416 = 8
 
# Early Dial. 0 - no, 1 - yes
P422 = 0

# Dial Plan Prefix
P419 =

# Dial Plan. Maxlength = 128, default is allow all {x.}
P459 = {x.}

# Delayed Call Forward Wait Time. Default is 20 seconds, maxlength = 5 
P470 = 20

# Enable Call Features. 0 - no, 1 - yes.
P420 = 1

# Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
P434 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
P427 = 90

# Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
P428 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
P429 = 0

# Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
P430 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
P433 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
P431 = 0

# Enable 100rel. 0 - no, 1 - yes
P435 = 0

# Account Ring Tone. 0 - system ring tone, 1 - custom ring tone 1, 2 - custom ring tone 2, 3 - custom ring tone 3.
P423 = 0

# Send Anonymous. 0 - no, 1 - yes ((caller ID will be blocked if set to Yes)
P421 = 0

# Anonymous Call Rejection:     0 - no (default),  1 - yes  
P446 = 0

# Refer-To Uses Target Contact:  0 - no (default),  1 - yes 
P469 = 0

# Auto Answer. 0 - no, 1 - yes, 2 - Intercom/Paging
P425 = 0

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 3 - GSM, 4 - G.723.1, 8 - PCMA, 
# 9 - G.722, 18 - G.729A/B, 98 - iLBC

# Currently only PCMU/PCMA, GSM, G.723, G.729 and G.726-32 supported, will add others in the future 

# First codec.
P451 = 0

# Second codec. 
P452 = 8

# Third codec.
P453 = 4

# Forth codec. 
P454 = 18

# Fifth codec.
P455 = 3

# Sixth codec.
P456 = 2

# Seventh codec.
P457 = 0

# Eighth codec.
P458 = 0

# Preferred Video Codec:   99 - H.264, 34 - H.263 103 - H.263+ (1998)
# Choice 1
P464 = 99

# Choice 2
P465 = 34

# Jitter Delay: 0 - Medium, 1 - Low, 2 - High
P467 = 0 

# Enable Video: 0 - No, 1 - Yes
P461 = 1

# H.264 payload type: between 96 ~ 127, default = 99
P462 = 99

# H.263+ (1998) payload type: between 96 ~ 127, default = 103
P473 = 103

# SRTP Mode: Disabled - 0, Enabled but not forced - 1, Enabled and forced - 2
P443 = 0

# Special Feature.    100 - Standard, 101 - Nortel MCS, 102 - BroadSoft, 104 - Sonus, 108 - CBCOM, 109 - RNK
P424 = 100

########################################################################
# SIP Account 3 Settings
########################################################################

# Account Active (In Use). 0 - no, 1 - yes
P501 = 0

# Account Name
P517 =

# SIP Server
P502 =

# Outbound Proxy Server
P503 =

# SIP User ID
P504 =

# Authenticate ID
P505 =

# Authenticate Password
P506 =

# Display Name (John Doe)
P507 =

# Use DNS SRV. 0 - No, 1 - Yes.
P508 = 0

# User ID is phone. "user=phone". 0 - no, 1 - yes
P509 = 0

# SIP Registration. 0 - no, 1 - yes
P510 = 1

# Unregister on Reboot. 0 - no, 1 - yes
P511= 0

# Register Expiration (in minutes. default 1 hour, max 45 days)
P512 = 60

# Registration Retry Wait Time (in seconds. Between 1-3600, default is 20)
P571 = 20

# SIP Local port (default 5064)
P513 = 5064

# NAT Traversal. 0 - yes, 1 - no, 2 - No, but send keep-alive
P514 =

# Subscribe MWI. (Whether or not send SUBSCRIBE for Message Waiting Indication) 0 - no, 1 - yes
P515 = 0

# Proxy Require
P518 =

# SIP Compact Header. 0 - no, 1 - yes
P572 = 0

# Voice Mail UserID (User ID/extension for 3rd party voice mail system)
P526 =
 
# Send DTMF. 8 - in audio, 1 - via RTP, 2 - via SIP INFO, 11 - In Audio & RTP & SIP INFO
# 9 - In Audio & RTP, 10 - IN Audio & SIP INFO, 3 - RTP & SIP INFO
P516 = 8

# Early Dial. 0 - no, 1 - yes
P522 = 0

# Dial Plan Prefix
P519 =

# Dial Plan: Maxlength = 128, default is allow all {x.}
P559 = {x.}

# Delayed Call Forward Wait Time. Default is 20 seconds, maxlength = 5 
P570 = 20

# Enable Call Features. 0 - no, 1 - yes.
P520 = 1

# Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
P534 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
P527 = 90

# Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
P528 =

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
P529 =

# Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
P530 =

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
P531 =

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
P532 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
P533 = 1

# Enable 100rel. 0 - no, 1 - yes
P535 = 0

# Account Ring Tone. 0 - system ring tone, 1 - custom ring tone 1, 2 - custom ring tone 2, 3 - custom ring tone 3.
P523 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - no, 1 - yes
P521 = 0

# Anonymous Call Rejection:     0 - no (default),  1 - yes 
P546 = 0

# Refer-To Uses Target Contact:  0 - no (default),  1 - yes 
P569 = 0

# Auto Answer. 0 - no, 1 - yes, 2 - Intercom/Paging
P525 = 0

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 3 - GSM, 4 - G.723.1, 8 - PCMA, 
# 9 - G.722, 18 - G.729A/B, 98 - iLBC

# Currently only PCMU/PCMA, GSM, G.723, G.729 and G.726-32 supported, will add others in the future 

# First codec.
P551 = 0

# Second codec.
P552 = 8

# Third codec.
P553 = 4

# Forth codec.
P554 = 18

# Fifth codec.
P555 = 3

# Sixth codec.
P556 = 2

# Seventh codec.
P557 = 0

# Eighth codec.
P558 = 0

# Preferred Video Codec:   99 - H.264, 34 - H.263, 103 - H.263+ (1998)
# Choice 1
P564 = 99

# Choice 2
P565 = 34

# Jitter Delay: 0 - Medium, 1 - Low, 2 - High
P567 = 0 

# Enable Video: 0 - No, 1 - Yes
P561 = 1

# H.264 payload type: between 96 ~ 127, default = 99
P562 = 99

# H.263+ (1998) payload type: between 96 ~ 127, default = 103
P573 = 103

# SRTP Mode: Disabled - 0, Enabled but not forced - 1, Enabled and forced - 2
P543 = 0

# Special Feature.    100 - Standard, 101 - Nortel MCS, 102 - BroadSoft, 104 - Sonus, 108 - CBCOM, 109 - RNK
P524 = 100

#################################################################################
# End User Settings. Please do not edit this section.
#################################################################################

# Web Access. 0 - HTTP, 1 - HTTPS
# P900 = 0  

# Web Port: HTTP default is 80 and HTTPS default is 443  
# P901 = 80

# End User Password
# P196 = 123

# DHCP/PPPoE support. 0 - yes, 1 - no
# P8 = 0

# DHCP hostname, alphabet, max. length is 32
# P146 = 

# DHCP domain, alphabet, max. length is 32
# P147 = 

# DHCP vendor class ID, alphabet, max. length is 32
# P148 = Grandstream GXV-3000 

# PPPoE support. PPPoE user ID
# P82 =

# PPPoE password
# P83 =

# PPPoE service name, max. length is 64 alpabit
# P269 = 

# Preferred DNS server, four field, octet digits
# P92 =  
# P93 = 
# P94 = 
# P95 = 

# Static IP Address. Ignore if DHCP or PPPoE is used
#P9 = 192
#P10 = 168
#P11 = 0
#P12 = 1

# Subnet mask. Ignore if DHCP or PPPoE is used
#P13 = 255
#P14 = 255
#P15 = 255
#P16 = 0

# Default Router. Ignore if DHCP or PPPoE is used
#P17 = 192
#P18 = 168
#P19 = 1
#P20 = 1

# DNS 1. Ignore if DHCP or PPPoE is used
#P21 = 192
#P22 = 168
#P23 = 0
#P24 = 1

# DNS 2. Ignore if DHCP or PPPoE is used
#P25 = 0
#P26 = 0
#P27 = 0
#P28 = 0

#----------------------------------------------------------------------------------
# End User Time settings
#----------------------------------------------------------------------------------

# Time Zone. Offset in minutes to GMT.
# option value = 0	GMT-12:00 (International Date Line West)
# option value = 60     GMT-11:00 (Midway Island, Samoa)
# option value = 120    GMT-10:00 (US Hawaiian Time)
# option value = 180    GMT-9:00  (US Alaska Time)
# option value = 240    GMT-8:00  (US Pacific Time, Los Angeles)
# option value = 300    GMT-7:00  (US Mountain Time, Denver)
# option value = 360    GMT-6:00  (US Central Time, Chicago)
# option value = 420    GMT-5:00  (US Eastern Time, New York), --- Default ---
# option value = 450    GMT-4:30  (Venezuela)
# option value = 480    GMT-4:00  (Atlantic Time, Quebec)
# option value = 510    GMT-3:30  (Newfoundland)
# option value = 540    GMT-3:00  (Greenland)
# option value = 600    GMT-2:00  (Mid-Atlantic)
# option value = 660    GMT-1:00  (Azores, Cape Verdi Is.)
# option value = 720    GMT 0:00  (London, Dublin, Edinburgh, Lisbon, Casablanca, Monrovia)
# option value = 780    GMT+1:00  (Paris, Amsterdam, Berlin, Rome, Vienna, Madrid, Warsaw, Brussels)
# option value = 840    GMT+2:00  (Israel, Cairo, Athens, Helsinki, Istanbul, Bucuresti)
# option value = 900    GMT+3:00  (Moscow, Kuwait, Baghdad, Nairobi)
# option value = 930    GMT+3:30  (Tehran)
# option value = 960    GMT+4:00  (Abu Dhabi, Baku)
# option value = 990    GMT+4:30  (Kabul)
# option value = 1020   GMT+5:00  (Islamabad, Ekaterinburg, Karachi, Tashkent)
# option value = 1050   GMT+5:30  (Calcutta, Chennai, Mumbai, New Delhi)
# option value = 1065   GMT+5:45  (Kathmandu)
# option value = 1080   GMT+6:00  (Almaty, Astana, Dhaka, Novosibirsk)
# option value = 1110   GMT+6:30  (Rangoon)
# option value = 1140   GMT+7:00  (Bankok, Jakarta, Hanoi, Krasnoyarsk)
# option value = 1200   GMT+8:00  (Beijing, Singapore, Taipei, Kuala Lumpur, Irkutsk, Perth)
# option value = 1260   GMT+9:00  (Japan, Korea, Yakutsk)
# option value = 1290   GMT+9:30  (Adelaide, Darwin)
# option value = 1320   GMT+10:00 (Brisbane, Sydney, Melbourne, Canberra, Guam, Hobart)
# option value = 1380   GMT+11:00 (Magadan, Solomon Is., New Caledonia)
# option value = 1440   GMT+12:00 (Auckland, Wellington, Fiji)
# option value = 1500   GMT+13:00 (Nuku'alofa)
#---------------------------------------------------------------------------------------
P64 = 420

# Allow DHCP Option 2 to override Time Zone setting. 0 - No, 1 - Yes.
# When set to Yes(1), it will override the configured Time Zone setting if available. 
P143 = 0

# Daylight Savings Time. 0 - no, 1 - yes
P75 = 0

# Optional Rule: 
# If Daylight Saving Time is selected (P75 = 1), optional rule will allow automatically time ajustment based on the configured rule
# Maxlength = 33, default is North America or US Daylight Saving Time Schecule: value="3,2,7,2,0;11,1,7,2,0;60"
P246 = 3,2,7,2,0;11,1,7,2,0;60

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour
P122 = 0

# Date Display Format. 0 - Year-Month-Day, 1 - Month-Day-Year, 2 - Day-Month-Year
P102 = 0

# Display Clock instead of Date. 0 - no, 1 - yes
P123 = 0

#----------------------------------------------------------------------------------
# End User LCD settings
#----------------------------------------------------------------------------------

# Disable SIP User Display:     0 - no (Default),  1 - yes
P940 = 0 

# Disable IP Address Display:   0 - no (Default),  1 - yes
P941 = 0 

# LCD Screen Saver Start Interval: in seconds, 0 means screen saver is off, max. length is 5
P913 = 60

# LCD Screen Saver Refresh Interval: in seconds. from 1-3600, default is 10, controls the time of screensaver image displayed on LCD.
P937 = 10

# LCD Auto Power Off Interval: in seconds, 0 means LCD will be always on, max. length is 5
P909 = 0

# LCD Brightness: max. length is 5, default is 128
P910 = 128

# LCD Contrast: max. length is 5, default is 128
P911 = 128

# LCD Chroma Saturation: max. length is 5, default is 128
P912 =128

# LCD Text Color:   maxlength=3 size=5
# Red (0-255) 
P930 = 255 
# Green (0-255)
P931 = 255
# Blue (0-255) 
P932 = 255       

# LCD Background Color: value is 0 to 255
# Red
P906 = 0
# Green
P907 = 0 
# Blue
P908 = 0

# OSD Text Color: 
# value = 1  Blue
# value = 2  Black
# value = 3  Purple
# value = 4  Dark Blue
# value = 5  Green
# value = 6  Red
# value = 7  Olive
# value = 8  Light Grey
# value = 12 Yellow
# value = 15 White
P922 = 15                   

# PIP Position:
# value=0  Top Left
# value=1  Top Right
# value=2  Bottom Left
# value=3  Bottom Right
P936 = 0

# Camera Zoom Mode:
# value = 0   1.0:1 (wide and default)
# value = 1   1.1:1
# value = 2   1.2:1
# value = 3   1.3:1
# value = 4   1.4:1
# value = 5   1.5:1
# value = 6   1.6:1
# value = 7   1.7:1
# value = 8   1.8:1
# value = 9   1.9:1
# value = 10  2.0:1 <optical tele)
# value = 11  2.2:1
# value = 12  2.4:1
# value = 13  2.6:1
# value = 14  2.8:1
# value = 15  3.0:1
# value = 16  3.2:1
# value = 17  3.4:1
# value = 18  3.6:1
# value = 19  3.8:1
# value = 20  4.0:1 (digital tele)
P914 = 0 

# Camera Exposure:    Default: 0 = auto
# value = 0   Auto
# value = 5   Very Bright
# value = 2   Bright
# value = 6   Less Bright I
# value = 7   Less Bright II
# value = 8   Less Bright II
# value = 1   Normal
# value = 9   Less Dim I
# value = 10  Less Dim II
# value = 11  Less Dim III
# value = 3   Dim
# value = 12  Less Dark
# value = 4   Dark
# value = 13  Very Dark
P915 = 0

# Camera Color Mode:     0 = Color mode (Default), 1 = Monochrome
P919 = 0

# Camera White Balance:  0 = auto (Default), 1 = fixed
P920 = 0 

# Camera Lens Correction: 0 = no, 1 = yes (Default)
P926 = 1

# TV Output:  0 = off (Default)
# value = 0   Off
# value = 1   NTSC
# value = 2   PAL-BDGHI
# value = 3   PAL-M/PALSA
# value = 4   PAL-Nc/PALSA
P916 = 0
 
